[Information]
This is a shopping list, only a few items may apply to any particular machine

The format of the text is important, careless editing this of file may cause 
sections to be incorrectly concatenated or missed

--------------------------------------------------------
|Group        |Tool Description       |Tag |Cost Group |
|-------------|-----------------------|----|-----------|
|Cutting      |Oxy-Fuel               |CT1 |1          |
|             |Air Plasma             |CT2 |1          |
|             |Hi-Def Plasma          |CT3 |2          |
|             |Router                 |CT4 |2          |
|             |Water Jet              |CT5 |3          |
|             |Laser                  |CT6 |3          |
|             |Spare                  |CT7 |3          |
--------------------------------------------------------
|Marking      |Plasma, separate Tool  |MT1 |1          |
|             |Laser, part of CT6     |MT2 |3          |
|             |Powder                 |MT3 |1          |
|             |Scribe                 |MT4 |1          |
|             |Inkjet                 |MT5 |1          |
|             |Pneumatic              |MT6 |1          |
|             |Router                 |MT7 |1          |
--------------------------------------------------------
|Bevelling    |Bevel Plasma           |BT1 |2          |
|             |Bevel Oxy-Fuel         |BT2 |4          |
--------------------------------------------------------
|Printing     |Ink Jet                |PT1 |2          |
|             |Pneumatic              |PT2 |2          |
--------------------------------------------------------
|Drill/Tap    |Drill			      |DT1 |1          |
|/Punch       |Punch                  |DT2 |1          |
|             |Tapping                |DT3 |3          |
|             |Centre Punch           |DT4 |1          |
|             |Spot Drill			  |DT5 |1          |	 
--------------------------------------------------------
|Special      |Null Tool              |NT0 |1          |
|             |Vaporize               |NT1 |3          |
|             |Size Adjuster          |NT2 |1          |
--------------------------------------------------------
          
[Tool Names]          
CT1=Oxy-Fuel
CT2=Air Plasma
CT3=Hi-Def Plasma
CT4=Router
CT5=Water Jet
CT6=Laser
CT7=Spare
MT1=Plasma
MT2=Laser
MT3=Powder
MT4=Scribe
MT5=Inkjet
MT6=Pneumatic
MT7=Router
BT1=Bevel Plasma
BT2=Bevel Oxy-Fuel
PT1=Ink Jet
PT2=Pneumatic
DT1=Drill
DT2=Punch
DT3=Tapping
DT4=Centre Punch
DT5=Spot Drill
NT0=Null Tool
NT1=Vaporizing          
NT2=Size Adjuster

[Tool Items]
TI00=Sheet Thickness
TI01=Post Number,I
TI02=Edge Approach
TI03=Feed Rate
TI04=Kerf Value
TI05=Kerf Code,I
TI06=Pierce Size
TI07=Pierce Delay
TI08=Arc Slow Radius
TI09=Arc Slow Factor
TI10=Arc Slow Min %
TI11=Corner Slow Angle
TI12=Corner Slow In Distance
TI13=Corner Slow Out Distance
TI14=Corner Slow Factor
TI15=Corner Slow Min %
TI16=Height Control Min Feed
TI17=Height Control Lock Distance
TI18=Height Control Unlock Distance
TI19=Voltage,I
TI20=Current,I
TI21=Ignore Size
TI22=Text Size
TI23=Cross Size
TI24=Selection Delay
TI25=Tool On Delay
TI26=Offset Value
TI27=Preheat Delay
TI28=Tool Off Delay
TI29=Traverse Feed
TI30=Power
TI31=Duty Cycle %
TI32=Tool Lower Time
TI33=Tool Raise Time
TI34=Number Of Heads,I
TI35=Pierce Program,I
TI36=S value
TI37=P value
TI38=Q value
TI39=T value
TI40=R value
TI41=Initial Feed Rate
TI42=Maximum Beam Travel
TI43=Gas Pressure
TI44=Drill Pierce Hole,B
TI45=Text Width Factor
TI46=Laser Table,W
TI47=Traverse Rate
TI48=Corner Cooling Time
TI49=Corner Cool Angle
TI50=Positioning Height
TI51=Operating Height
TI52=Enable Height Control,T
TI53=Enable Pierce Height Measurement,T
TI54=Leadin Technology,I 
TI55=Cutting Technology,I 
TI56=Vaporising Technology,I
TI57=Point Marking Technology,I
TI58=Engraving Technology,I
TI59=Tool On Program,I
TI60=Tool Off Program,I
TI61=Sheet Rail
TI62=Sheet Beam
TI63=Rapid Pierce,B
TI64=Corner Cool Program,I
TI65=Autoload Enabled
TI66=Corner Cool Distance
TI67=Feed Code,I
TI68=Leadin Feed Code,I
TI69=Reduced Speed Leadin,B
TI70=Kerf Cancel Distance
TI71=First Cutting Tool
TI72=Parameter Set,I
TI73=Cutting Mode,I
TI74=Mark Pierce,B
TI75=Tool Stays Down For Traverse,B
TI76=Purge Delay,B
TI77=Head,I
TI79=Pulsed Cutting,B
TI80=Pulsed Piercing,B
TI81=D value,I
TI82=E value,I
TI83=Gas Type,I
TI84=Pierce Height
TI85=Flow Rate(1),I
TI86=Flow Rate(2),I
TI87=Flow Rate(3),I
TI88=Flow Rate(4),I
TI89=Flow Rate(5),I
TI90=Flow Rate(6),I
TI91=Height Control Min Radius
TI92=Focus
TI93=Sensor Type,I
TI94=Frequency,I
TI95=Pierce Type,I
TI96=Cut Type,I
TI97=Acceleration
TI98=Deceleration
TI99=Maximum Height
TI100=Pulse Mode,I
TI101=Operating Height
TI102=Focus
TI103=Lead In Height Control Lock Distance
TI104=Enable Pierce Delay,B
TI105=Lathe Pit Rail Origin
TI106=Lathe Pit Beam Origin
TI107=Lathe Pit Positioning Height
TI108=Purge Head,B
TI109=Purge Rail Position
TI110=Purge Beam Position
TI111=Flush Delay
TI112=Mark Centre,B
TI113=Lathe Pit Rail Finish
TI114=Lathe Pit Beam Finish
TI115=Printer Model,I
TI116=Suppress Feed Rate,B
TI117=Trap Door Minimum Size
TI118=Trap Door maximum Size
TI119=Pierce Gas,I
TI120=Cutting Gas,I
TI121=Pierce Pulse Mode,I
TI122=Cut Pulse Mode,I
TI123=Plunge Rate
TI124=Spindle Speed,I
TI125=Number of Passes,I
TI126=Maximum Cut Depth/Pass
TI127=Last Cut Depth
TI128=Marking Depth
TI129=Cut Through Sheet,B
TI130=Extra Cut Through Depth
TI131=Pierce Circle,B
TI132=Nesting Margin
TI133=Diameter
TI134=Bottom/Peck Dwell
TI135=Cycle Mode,I
TI136=Peck Depth
TI137=External Coolant,B
TI138=Material Number,I
TI139=Small Contour Minimum
TI140=Small Contour Maximum
TI141=Medium Contour Minimum
TI142=Medium Contour Maximum
TI143=Large Contour Minimum
TI144=Large Contour Maximum
TI145=Small Contour Rounding,B
TI146=Large Contour Rounding,B
TI147=Vaporise,B
TI148=SprintLas,B
TI149=Rule Type,W
TI150=Small Contour Round Radius
TI151=Small Contour Vaporise,B
TI152=Large Contour Round Radius
TI153=Large Contour Vaporise,B
TI154=RipCut Standoff
TI155=Reduced Acceleration,B
TI156=Small Contour Slow Start,B
TI157=Large Contour Slow Start,B
TI158=Small Contour Slow %
TI159=Large Contour Slow %
TI160=Height Control Margin
TI161=Sheet Measuring Distance

[Tool Conditions]
CC01=Contour Area
CC02=Contour Length
CC03=Contour Extents
CC04=Bevel Angle
CC05=Current
CC06=Code
CC07=Leadin Code
CC08=Line Length
CC09=Arc Radius
CC10=Circle Radius
CC11=Piercing,I
CC12=Cutting,I
CC13=Rules,W

[Features]
FT0=WADR2 Format
FT1=Vaporize
FT2=Speed Reduction Leadin
FT3=Comb.Leadin Same Speed
FT4=Shuttercontrol
FT5=Exact Stop on Leadin
FT6=Use Subroutines at Any Angle
FT7=Sheet Loading
FT8=Use Subroutines at Any Quadrant
FT9=Z Axis Substitution for Y Axis
FT*10=Low Memory Auto Reload
FT*11=Unix File Format
FT*12=Return Home At End Of Sheet
FT*13=Autoload After Return Home
FT*14=Gold or Platino
FT*15=Scrap Collection
FT*16=Sheet Location
FT*17=Kerf Leads
FT*18=Stop On Tool Change 
FT*19=Double Line Printing
FT*20=Kerf All 
FT*21=Change Torch Spacing at Any Position
FT*22=Arc Voltage Height Sensing
FT*23=Part Collection
FT*24=Add Sheet Format
FT*25=Go Home On Tool Change 
FT*26=Output Actual Feed Rate
FT*26=Omit Program Number
FT*27=Set Origin
FT*28=Block Number for Tool Change
FT*29=Reverse Tables
FT*30=Return Home After Last Sheet

[Tool Strings]
TS00=Active Tools
