; USBDrv.inf
;For win98/2k/xp/2003/vista

;--------- Version Section ---------------------------------------------------

[Version]
LayoutFile= Layout.inf, Layout1.inf, Layout2.inf
Signature="$CHICAGO$"
Provider=%ProviderName%
Class=加密设备
ClassGUID={ff646f81-8def-11d2-9449-00105a075f6b}
DriverVer=12/29/2009,3.0
CatalogFile=SDT_S_DRV.cat

;--------- SourceDiskNames and SourceDiskFiles Section -----------------------

; These sections identify source disks and files for installation.  They are
; shown here as an example, but commented out.

[SourceDisksNames]
1 = "SDT Driver Disk","",,

[SourceDisksFiles]
USBDrv.sys = 1,,
samcoins.dll=1,,

[SourceDiskFiles.NT]
USBDrv.sys = 1,,
samcoins.dll=1,,
;--------- ClassInstall/ClassInstall32 Section -------------------------------

; Not necessary if using a standard class

; 9X Style
[ClassInstall]
Addreg=Class_AddReg

; NT Style
[ClassInstall32.NT]
Addreg=Class_AddReg

[Class_AddReg]
HKR,,,,%DeviceClassName%
HKR,,Icon,,"0"

;--------- DestinationDirs Section -------------------------------------------

[DestinationDirs]
USBDrv_Files_Driver = 10,System32\Drivers
Files_CoInstaller=11 ; 11 ; system dir (system32 for NT)


;--------- Manufacturer and Models Sections ----------------------------------

[Manufacturer]
%MfgName%=Mfg0

[Mfg0]
%DeviceDesc%=USBDrv_DDI, USB\VID_0400&PID_c35a

;---------- DDInstall Sections -----------------------------------------------
; --------- Windows 9X -----------------

; Experimentation has shown that DDInstall root names greater than 19 characters
; cause problems in Windows 98

[USBDrv_DDI]
CopyFiles=USBDrv_Files_Driver
AddReg=USBDrv_9X_AddReg
;Reboot

[USBDrv_9X_AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBDrv.sys

; --------- Windows NT -----------------

[USBDrv_DDI.NT]
CopyFiles=USBDrv_Files_Driver,Files_CoInstaller
AddReg = CoInstaller_AddReg
;Reboot

[CoInstaller_AddReg]
HKLM,System\CurrentControlSet\Control\CoDeviceInstallers, {ff646f81-8def-11d2-9449-00105a075f6b},0x00010008, "samcoins.dll,SDTSamUsbCoInstaller"
; above line uses the line continuation character (\)

[USBDrv_DDI.NT.Services]
Addservice = USBDrv, 0x00000002, USBDrv_AddService

[USBDrv_AddService]
DisplayName    = %SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\USBDrv.sys
LoadOrderGroup = Base

; --------- Files (common) -------------

[USBDrv_Files_Driver]
USBDrv.sys,,,2

;=====================================================================
; Copy files specific to NT platform (2000 / XP)
;=====================================================================
[Files_CoInstaller]
samcoins.dll,,,2


;--------- Strings Section ---------------------------------------------------

[Strings]
ProviderName="SDT"
MfgName="SDT Telecom"
DeviceDesc="SDT USB设备"
DeviceClassName="密码设备"
SvcDesc="USBDrv.Sys WDM USB client"
